IFC building model
Schema: "IFC4"
Description: "IFC4"
File name: "200429_Geocollect_Verlegeschema_3_mit_Schrift.IFC"
Time stamp: "2020-04-29T06:48:53"
Preprocessor: "SwIFC"
Originating system: "SolidWorks 2019"
Application: "SolidWorks 2019" version "19.0" identifier "SolidWorks" by Organization "SolidWorks" id "SW" description "SolidWorks"

People and organizations
  Person (no name given) of Organization ""
  Owner history of Person (no name given) of Organization "" | application "SolidWorks 2019" version "19.0" identifier "SolidWorks" by Organization "SolidWorks" id "SW" description "SolidWorks" | change ADDED | created 1588142933 (2020-04-29T06:48:53Z) | last modified 1588142933 (2020-04-29T06:48:53Z) by Person (no name given) of Organization "" with "SolidWorks 2019" version "19.0" identifier "SolidWorks" by Organization "SolidWorks" id "SW" description "SolidWorks"

Units
  LENGTHUNIT: METER
  AREAUNIT: SQUARE_METER
  VOLUMEUNIT: CUBIC_METER

Spatial structure
IFCPROJECT "Default Project"
  IFCSITE "Default Site" | latitude 0° 0′ 0″ | longitude 0° 0′ 0″ | elevation above sea level 0.0000000000000000000
    IFCBUILDING "Default Building"
      IFCBUILDINGSTOREY "Default Storey" | elevation 0.0000000000000000000
        contains 1 element
          1 x IFCELEMENTASSEMBLY | object type "200429_Geocollect_Verlegeschema_3_mit_Schrift" | names: "200429_Geocollect_Verlegeschema_3_mit_Schrift" | parts: 23 IFCBEAM, 10 IFCBUILDINGELEMENTPROXY, 1 IFCCURTAINWALL | property sets: SolidWorks Custom Properties, PSet_Mass_Property

Property sets
  SolidWorks Custom Properties | properties | on 20 objects (12 IFCBEAM, 8 IFCBUILDINGELEMENTPROXY)
    Burst pressure = "12,3 bar" (IFCLABEL)
    Description = "Geothermal heat collector" (IFCLABEL)
    Internal Volume / liquid capacity = "1,75l" (IFCLABEL)
    Manufacturer = "GeoCollect (TM)" (IFCLABEL)
    Material = "Polypropylen" (IFCLABEL)
    Model = "GC 2" (IFCLABEL)
    Nominal power (depending on operating conditions) = "99,45 W" (IFCLABEL)
    Operating Temperature range = "-15 degC to +40 degC" (IFCLABEL)
    Operating pressure = "3 bar" (IFCLABEL)
    Outer Dimensions = "890 x 350 x 40 mm^3" (IFCLABEL)
    Pressure loss (single modul) = "ca. 150 Pa" (IFCLABEL)
    Temporary Operating Temperature range = "-20 degC to +60 degC" (IFCLABEL)
    Test pressure = "6 bar" (IFCLABEL)
    Weight = "1900.00" (IFCLABEL)
  SolidWorks Custom Properties | properties | on 4 objects (4 IFCBEAM)
    Angle = "90 deg" (IFCLABEL)
    Description = "Elbow DN 32" (IFCLABEL)
    Material = "Polypropylen PP-R" (IFCLABEL)
    Pressure stage = "PN20" (IFCLABEL)
    Side A Inner diameter = "32 mm" (IFCLABEL)
    Side A Outer diameter = "46 mm" (IFCLABEL)
    Side B Inner diameter = "32 mm" (IFCLABEL)
    Side B Outer diameter = "46 mm" (IFCLABEL)
    Weight = "48.81" (IFCLABEL)
  SolidWorks Custom Properties | properties | on 4 objects (3 IFCBEAM, 1 IFCBUILDINGELEMENTPROXY)
    Description = "Reduction d32-DN25" (IFCLABEL)
    Length = "38.5 mm" (IFCLABEL)
    Material = "Polypropylen PP-R" (IFCLABEL)
    Pressure stage = "PN20" (IFCLABEL)
    Side A Inner diameter = "17 mm" (IFCLABEL)
    Side A Outer diameter = "32 mm" (IFCLABEL)
    Side B Inner diameter = "25 mm" (IFCLABEL)
    Side B Outer diameter = "36 mm" (IFCLABEL)
    Weight = "20.19" (IFCLABEL)
  SolidWorks Custom Properties | properties | on 2 objects (2 IFCBEAM)
    Description = "Pipe d32" (IFCLABEL)
    Inner diameter = "26.2 mm" (IFCLABEL)
    Length = "400 mm" (IFCLABEL)
    Material = "Polypropylen PP-R" (IFCLABEL)
    Outer diameter = "32 mm" (IFCLABEL)
    Weight = "95.23" (IFCLABEL)
  SolidWorks Custom Properties | properties | on 2 objects (1 IFCBEAM, 1 IFCCURTAINWALL)
    Description = "Connection hose d25" (IFCLABEL)
    Inner diameter = "20.4 mm" (IFCLABEL)
    Length = "variable, depending on site demands" (IFCLABEL)
    Material = "Polypropylen PP-R" (IFCLABEL)
    Outer diameter = "25 mm" (IFCLABEL)
    Weight = "1429.91" (IFCLABEL)
  SolidWorks Custom Properties | properties | on 2 objects (1 IFCBEAM, 1 IFCBUILDINGELEMENTPROXY)
    Description = "Connection hose d25" (IFCLABEL)
    Inner diameter = "20.4 mm" (IFCLABEL)
    Length = "variable, depending on site demands" (IFCLABEL)
    Material = "Polypropylen PP-R" (IFCLABEL)
    Outer diameter = "25 mm" (IFCLABEL)
    Weight = "7.36" (IFCLABEL)
  SolidWorks Custom Properties | properties | on 1 object (1 IFCELEMENTASSEMBLY)
    Follow design instructions at = "https://www.geocollect.de/" (IFCLABEL)
    Forbidden is = "Overbuilding, sealed surfaces above collectors, dry gravel or rocky surrounding" (IFCLABEL)
    Further planning details = "https://www.geocollect.de/" (IFCLABEL)
    Heat extraction rate = "2 kW" (IFCLABEL)
    Maximum slope = "15 %" (IFCLABEL)
    Minimum distance to light wells = "1 m" (IFCLABEL)
    Minimum distance to other media = "0,5 m" (IFCLABEL)
    Minimum distance to property line = "1 m" (IFCLABEL)
    Minimum distance to sewer pipes = "0,3 m" (IFCLABEL)
    Minimum distance to walls = "1 m" (IFCLABEL)
    Minimum distance to water pipes = "1 m" (IFCLABEL)
    Minimum installation temperature = ">5 °C, ideal: >10°C" (IFCLABEL)
    Minimum required Area = "7 m²" (IFCLABEL)
    Surrounding soil = "Sand, 35 cm around collectors" (IFCLABEL)
    Variant Nr. = "3" (IFCLABEL)
    Volume flow rate at 3K temp. difference = "10 l/min" (IFCLABEL)
    maximum allowed plant root depth from above = "0,8 m" (IFCLABEL)
  PSet_Mass_Property | properties | on 1 object (1 IFCELEMENTASSEMBLY)
    Area Measure = 20.13664030488116197 (IFCAREAMEASURE) [SQUARE_METER]
    Mass Measure = 41.34102538352102130 (IFCMASSMEASURE)
    Volume Measure = 0.2068777758710786674 (IFCVOLUMEMEASURE) [CUBIC_METER]