IFC building model
Schema: "IFC4"
Description: "IFC4"
File name: "200708_Geocollect_Verlegeschema_2_mitSchriftzug.IFC"
Time stamp: "2020-07-08T09:47:54"
Preprocessor: "SwIFC"
Originating system: "SolidWorks 2019"
Application: "SolidWorks 2019" version "19.0" identifier "SolidWorks" by Organization "SolidWorks" id "SW" description "SolidWorks"

People and organizations
  Person (no name given) of Organization ""
  Owner history of Person (no name given) of Organization "" | application "SolidWorks 2019" version "19.0" identifier "SolidWorks" by Organization "SolidWorks" id "SW" description "SolidWorks" | change ADDED | created 1594201674 (2020-07-08T09:47:54Z) | last modified 1594201674 (2020-07-08T09:47:54Z) by Person (no name given) of Organization "" with "SolidWorks 2019" version "19.0" identifier "SolidWorks" by Organization "SolidWorks" id "SW" description "SolidWorks"

Units
  LENGTHUNIT: METER
  AREAUNIT: SQUARE_METER
  VOLUMEUNIT: CUBIC_METER

Spatial structure
IFCPROJECT "Default Project"
  IFCSITE "Default Site" | latitude 0° 0′ 0″ | longitude 0° 0′ 0″ | elevation above sea level 0.0000000000000000000
    IFCBUILDING "Default Building"
      IFCBUILDINGSTOREY "Default Storey" | elevation 0.0000000000000000000
        contains 1 element
          1 x IFCELEMENTASSEMBLY | object type "200708_Geocollect_Verlegeschema_2_mitSchriftzug" | names: "200708_Geocollect_Verlegeschema_2_mitSchriftzug" | parts: 9 IFCBEAM, 8 IFCBUILDINGELEMENTPROXY | property sets: SolidWorks Custom Properties, PSet_Mass_Property

Property sets
  SolidWorks Custom Properties | properties | on 10 objects (6 IFCBUILDINGELEMENTPROXY, 4 IFCBEAM)
    Burst pressure = "12.3 bar" (IFCLABEL)
    Density absorber material (PP-R) = "898 kg / m^3" (IFCLABEL)
    Description = "Geothermal absorber" (IFCLABEL)
    Inner heat exchanger surface of a module = "0.8 m^2" (IFCLABEL)
    Internal Volume / Fill amount = "1.75 l" (IFCLABEL)
    Manufacturer = "GeoCollect (R)" (IFCLABEL)
    Material = "Polypropylen" (IFCLABEL)
    Model = "GC 2" (IFCLABEL)
    Nominal power (depending on operating conditions) = "99.45 W" (IFCLABEL)
    Operating Temperature limits = "-15 degC to +40 degC" (IFCLABEL)
    Outer Dimensions = "890 x 350 x 40 mm^3" (IFCLABEL)
    Outer heat exchanger surface of a module = "2 x 0.31 m^2" (IFCLABEL)
    Pressure loss per modul = "ca. 150 Pa" (IFCLABEL)
    Temporary Operating Temperature limits = "-20 degC to +60 degC" (IFCLABEL)
    Test pressure = "6 bar" (IFCLABEL)
    Weight / g = "1900.00" (IFCLABEL)
    Working pressure = "0.8 - 1.2 bar" (IFCLABEL)
  SolidWorks Custom Properties | properties | on 2 objects (2 IFCBEAM)
    Description = "Reduction d32-DN25" (IFCLABEL)
    Length = "38.5 mm" (IFCLABEL)
    Material = "Polypropylen PP-R" (IFCLABEL)
    Pressure stage = "PN20" (IFCLABEL)
    Side A Inner diameter = "17 mm" (IFCLABEL)
    Side A Outer diameter = "32 mm" (IFCLABEL)
    Side B Inner diameter = "25 mm" (IFCLABEL)
    Side B Outer diameter = "36 mm" (IFCLABEL)
    Weight = "20.19" (IFCLABEL)
  SolidWorks Custom Properties | properties | on 2 objects (1 IFCBEAM, 1 IFCBUILDINGELEMENTPROXY)
    Angle = "90 deg" (IFCLABEL)
    Description = "Elbow DN 32" (IFCLABEL)
    Material = "Polypropylen PP-R" (IFCLABEL)
    Pressure stage = "PN20" (IFCLABEL)
    Side A Inner diameter = "32 mm" (IFCLABEL)
    Side A Outer diameter = "46 mm" (IFCLABEL)
    Side B Inner diameter = "32 mm" (IFCLABEL)
    Side B Outer diameter = "46 mm" (IFCLABEL)
    Weight = "48.81" (IFCLABEL)
  SolidWorks Custom Properties | properties | on 1 object (1 IFCELEMENTASSEMBLY)
    Follow design instructions at = "https://www.geocollect.de/" (IFCLABEL)
    Forbidden is = "Overbuilding, sealed surfaces above collectors, dry gravel or rocky surrounding" (IFCLABEL)
    Installation to distributor = "parallel" (IFCLABEL)
    Layout scheme = "2" (IFCLABEL)
    Max. distance to brine distributor = "50 m" (IFCLABEL)
    Max. slope = "15 %" (IFCLABEL)
    Min. distance to light wells = "1 m" (IFCLABEL)
    Min. distance to other media = "0.5 m" (IFCLABEL)
    Min. distance to property line = "1 m" (IFCLABEL)
    Min. distance to sewer pipes = "0.3 m" (IFCLABEL)
    Min. distance to walls = "1 m" (IFCLABEL)
    Min. distance to water pipes = "1 m" (IFCLABEL)
    Min. installation temperature = ">5 deg C, ideal: >10 deg C" (IFCLABEL)
    Min. required Area = "7 m^2" (IFCLABEL)
    Nominal heat extraction rate at 1800 working hrs / a = "1 kW *when installed properly, see: https://www.geocollect.de/" (IFCLABEL)
    Surrounding soil = "Sand (max grain size: 2mm): 35cm around absorber units" (IFCLABEL)
    Volume flow rate at 3K temp. difference = "5 l/min" (IFCLABEL)
    max. allowed plant root depth from above = "0.8 m" (IFCLABEL)
  SolidWorks Custom Properties | properties | on 1 object (1 IFCBEAM)
    Description = "Connection hose d25" (IFCLABEL)
    Inner diameter = "20.4 mm" (IFCLABEL)
    Length = "variable, depending on site demands" (IFCLABEL)
    Material = "Polypropylen PP-R" (IFCLABEL)
    Outer diameter = "25 mm" (IFCLABEL)
    Weight = "7.36" (IFCLABEL)
  SolidWorks Custom Properties | properties | on 1 object (1 IFCBEAM)
    Description = "Connection hose d32" (IFCLABEL)
    Inner diameter = "26.2 mm" (IFCLABEL)
    Length = "100 mm" (IFCLABEL)
    Material = "Polypropylen PP-R" (IFCLABEL)
    Outer diameter = "32 mm" (IFCLABEL)
    Weight = "23.81" (IFCLABEL)
  SolidWorks Custom Properties | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Description = "Connection hose d25" (IFCLABEL)
    Inner diameter = "20.4 mm" (IFCLABEL)
    Length = "variable, depending on site demands" (IFCLABEL)
    Material = "Polypropylen PP-R" (IFCLABEL)
    Outer diameter = "25 mm" (IFCLABEL)
    Weight = "1429.91" (IFCLABEL)
  PSet_Mass_Property | properties | on 1 object (1 IFCELEMENTASSEMBLY)
    Area Measure = 10.01346794470890700 (IFCAREAMEASURE) [SQUARE_METER]
    Mass Measure = 20.59908963207310251 (IFCMASSMEASURE)
    Volume Measure = 0.1033593522343283777 (IFCVOLUMEMEASURE) [CUBIC_METER]