IFC building model
Schema: "IFC4"
Description: "IFC4"
File name: "201019_Standard-Hauseinführung_d75.IFC"
Time stamp: "2020-10-19T13:54:23"
Preprocessor: "SwIFC"
Originating system: "SolidWorks 2019"
Application: "SolidWorks 2019" version "19.0" identifier "SolidWorks" by Organization "SolidWorks" id "SW" description "SolidWorks"

People and organizations
  Person (no name given) of Organization ""
  Owner history of Person (no name given) of Organization "" | application "SolidWorks 2019" version "19.0" identifier "SolidWorks" by Organization "SolidWorks" id "SW" description "SolidWorks" | change ADDED | created 1603115663 (2020-10-19T13:54:23Z) | last modified 1603115663 (2020-10-19T13:54:23Z) by Person (no name given) of Organization "" with "SolidWorks 2019" version "19.0" identifier "SolidWorks" by Organization "SolidWorks" id "SW" description "SolidWorks"

Units
  LENGTHUNIT: METER
  AREAUNIT: SQUARE_METER
  VOLUMEUNIT: CUBIC_METER

Spatial structure
IFCPROJECT "Default Project"
  IFCSITE "Default Site" | latitude 0° 0′ 0″ | longitude 0° 0′ 0″ | elevation above sea level 0.000000000000000000
    IFCBUILDING "Default Building"
      IFCBUILDINGSTOREY "Default Storey" | elevation 0.000000000000000000
        contains 1 element
          1 x IFCELEMENTASSEMBLY | object type "201019_Standard-Hauseinführung_d75" | names: "201019_Standard-Hauseinführung_d75" | parts: 24 IFCBUILDINGELEMENTPROXY, 19 IFCBEAM, 1 IFCELEMENTASSEMBLY | property sets: SolidWorks Custom Properties, PSet_Mass_Property

Property sets
  SolidWorks Custom Properties | properties | on 66 objects (30 IFCBEAM, 29 IFCBUILDINGELEMENTPROXY, 6 IFCELEMENTASSEMBLY, 1 IFCACTUATOR)
  SolidWorks Custom Properties | properties | on 2 objects (1 IFCBEAM, 1 IFCBUILDINGELEMENTPROXY)
    Description = "Rubber Steel Sealing" (IFCLABEL)
    Inner diameter = "77 mm" (IFCLABEL)
    Material = "EPDM 60 Durometer" (IFCLABEL)
    Outer diameter = "127 mm" (IFCLABEL)
    Pressure stage = "PN10-40" (IFCLABEL)
    Thickness = "4 mm" (IFCLABEL)
    Weight = "37.11" (IFCLABEL)
  SolidWorks Custom Properties | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Description = "Pipe d75" (IFCLABEL)
    Inner diameter = "61.4 mm" (IFCLABEL)
    Length = "variable length depending on site demands" (IFCLABEL)
    Material = "PE 100" (IFCLABEL)
    Outer diameter = "75 mm" (IFCLABEL)
    Pressure stage = "PN10" (IFCLABEL)
    SDR = "SDR 11" (IFCLABEL)
    Weight = "1118.93" (IFCLABEL)
  SolidWorks Custom Properties | properties | on 1 object (1 IFCELEMENTASSEMBLY)
    Description = "House lead-in / house connection" (IFCLABEL)
    House boring size = "150 mm" (IFCLABEL)
    In house connection = "Thread G 2'" (IFCLABEL)
    Material = "PE black, Steel" (IFCLABEL)
    Nominal Diameter = "d75" (IFCLABEL)
    Other sizes = "Other sizes possible on request" (IFCLABEL)
    Weight = "20753.33" (IFCLABEL)
  SolidWorks Custom Properties | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Description = "Threaded blind flange" (IFCLABEL)
    For pipe dimension = "d75" (IFCLABEL)
    Material = "1.0036 (S235JRG1)" (IFCLABEL)
    Thread type = "G 2'" (IFCLABEL)
    Weight = "3262.62" (IFCLABEL)
  SolidWorks Custom Properties | properties | on 1 object (1 IFCBEAM)
    DESIGN = "KSL 75-65-16-B-R14" (IFCLABEL)
    DESIGN1 = "Flansch-Kugelhahn Sphäroguss" (IFCLABEL)
    Description = "Ball valve DN 65" (IFCLABEL)
    Flange type = "DN 65" (IFCLABEL)
    Inner diameter = "65" (IFCLABEL)
    IsFastener = "1" (IFCLABEL)
    Length = "170 mm" (IFCLABEL)
    MASS = "12 kg" (IFCLABEL)
    MATERIAL = "Sphäroguss" (IFCLABEL)
    Material housing = "Steel" (IFCLABEL)
    Material sealing = "EPDM" (IFCLABEL)
    OMNICLASS23 = "23.27.31.15" (IFCLABEL)
    REFERENCE = "KSL75-65-16-B" (IFCLABEL)
    STANDARD = "DIN ISO 5211, DIN EN 1092-2 PN 16" (IFCLABEL)
    SUPPLIER = "BEE" (IFCLABEL)
    TRACEPARTS = "TRACEPARTS" (IFCLABEL)
    TYPE = "CATPART" (IFCLABEL)
    TraceParts.ClassPath = "BEE:32-04082016-088895" (IFCLABEL)
    TraceParts.InstanceId = "32-04082016-088895BTEIXUEDLXG4IEP66FDQ8ED89" (IFCLABEL)
    TraceParts.PartLanguage = "de" (IFCLABEL)
    TraceParts.PartNumber = "32-04082016-088895" (IFCLABEL)
    TraceParts.PartStatus = "Published" (IFCLABEL)
    TraceParts.PartStatusId = "" (IFCLABEL)
    TraceParts.PartTitle = "Flanschkugelhähne aus Sphäroguß, voller Durchgang, DN 25 - DN 150, PN 16, Baureihe KSL 75 - B" (IFCLABEL)
    TraceParts.PartVersion = "1.1.3" (IFCLABEL)
    Weight = "12995.76" (IFCLABEL)
  SolidWorks Custom Properties | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Description = "Loose flange" (IFCLABEL)
    For pipe dimension = "d75" (IFCLABEL)
    Inner diameter = "92 mm" (IFCLABEL)
    Material = "Polypropylen PP-R" (IFCLABEL)
    Outer diameter = "186 mm" (IFCLABEL)
    Thickness = "19 mm" (IFCLABEL)
    Weight = "331.84" (IFCLABEL)
  SolidWorks Custom Properties | properties | on 1 object (1 IFCBEAM)
    Description = "Welding Neck" (IFCLABEL)
    For pipe dimension = "d75" (IFCLABEL)
    Inner diameter = "66 mm" (IFCLABEL)
    Material = "PE hochdicht" (IFCLABEL)
    Outer diameter = "122 mm" (IFCLABEL)
    Thickness = "4.5 mm" (IFCLABEL)
    Weight = "208.25" (IFCLABEL)
  SolidWorks Custom Properties: 3 more contents on 3 objects not shown
  PSet_Mass_Property | properties | on 1 object (1 IFCELEMENTASSEMBLY)
    Area Measure = 1.511602253448486977 (IFCAREAMEASURE) [SQUARE_METER]
    Mass Measure = 20.75332990156823953 (IFCMASSMEASURE)
    Volume Measure = 0.006629440531725131272 (IFCVOLUMEMEASURE) [CUBIC_METER]